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Applicant


LYMAN BROS., INC.
Location


10288 S. Jordan Gateway #K




South Jordan, Salt Lake, UT 84095
Purpose
  Modification filed to add Amazonas 1 satellite as point of communication, and to use extended Ku-band frequency 13750-14000 MHz.

File No.


SES-MOD-20050927-01323
Call Sign


E030342
Latitude


 40  33 54 N

Longitude


111 54 14 W

Satellite


AMAZONAS 1

Transmit frequency

13750-14000 MHz

Polarization


Horizonal and Vertical




Maximum



Maximum
E.I.R.P.

Emissions
E.I.R.P.

Density

Frequency
36M0G7D
85.50

45.50

13750-14000 (MHz)
409KG7D
65.50                    45.40

13750-14000 (MHz)

